1. **TUJUAN**

Sebagai pedoman kerja untuk melakukan penyimpanan barang jadi.

1. **REFERENSI**

-

1. **PERSIAPAN**
   1. Forklift
   2. Stopper
   3. Cat anti rayap
   4. Terpal
2. **PELAKSANAAN**

Sebelum memindahkan barang ke area penyimpanan, pastikan barang jadi termasuk sisa potong sudah diberi sticker QC PASSED, End Cap dan terdapat identitas dengan jelas.

Barang jadi harus disimpan di tempat kering (tidak ada genangan air) dan terlindung dari sinar matahari langsung.

Untuk barang jadi yang dipacking dengan roll saat penyimpanan barang jadi harus ditempatkan pada palet terlebih dahulu kemudian susun pada rak sesuai item kelompoknya

Untuk barang jadi yang dipacking menggunakan haspel / bobbin, saat penyimpanan drum disusun pada posisi berdiri dan diberi jarak antar drum untuk memudahkan akses. Dan dapat ditumpuk sesuai dengan SM.08.01.01.

Apabila mengharuskan memindahkan barang jadi pada drum secara manual, maka pastikan pada saat mendorong tidak ada barang lain atau area yang rusak yang dapat merusak drum/barang jadi.

Area penyimpanan harus bebas dari lembap, kejatuhan, ketumpahan bahan kimia dan jauhkan dari tempat yang panas.

Pastikan barang disimpan sesuai kelompok area / lay out yang telah ditentukan

Apabila mengharuskan kabel disimpan di area terbuka / outdoor maka yang harus diperhatikan saat penyimpanan yaitu:

1. ***PURPOSE***

*As a working guideline for the storage of finished goods.*

1. ***REFERENCE***

*-*

1. ***PREPARATION***
2. *Forklift*
3. *Stopper*
4. *Anti-termite paint*
5. *Cover*
6. ***IMPLEMENTATION***
   1. *Before moving the goods to the storage area, make sure the finished goods including remaining goods has been add stickers QC PASSED, End Cap and there is an identity.*
   2. *Finished goods should be stored in a dry place (no puddles) and protected from direct sun.*
   3. *For finished goods packed with roll when will be stored of finished goods should be placed on the pallet first then stack on the shelf according to the item of the group.*
   4. *For finished goods using wooden drum / bobbin, when drum storage is arranged in standing position and spaced between drums for easy access. And can be stacked in accordance with SM.08.01.01.*
   5. *If required to move finished goods using drum manually, make sure that when pushing no other item or damaged area can damage the drum or products*
   6. *Storage areas shall be free of damp, fall, chemical spills and keep away from hot spots.*
   7. *Make sure the items are kept according to the group area*
   8. *If requiring cables to be stored in an open / outdoor area then that must be considered during storage are:*

* Barang jadi yang diperbolehkan disimpan outdoor hanya barang yang menggunakan packing drum.
* Lama penyimpanan tidak boleh lebih dari 2 bulan untuk menghindari kayu lapuk.
* Namun apabila mengharuskan penyimpanan lebih dari 2 bulan maka drum harus diberi cat anti rayap dan tutup barang jadi dengan menggunakan terpal.
* Simpan barang jadi pada permukaan keras (dicor atau paving blok) yang bebas dari genangan air.
* Hindari penyimpanan pada tanah langsung karena dapat membuat packing drum menjadi cepat lapuk dan rusak.
* Susunlah drum barang jadi sejajar dan dapat disusun ke atas sesuai dengan SM.08.01.01.
* Beri jarak antar drum agar mudah diakses.
* Dilakukan pengecekan berkala untuk memantau kondisi packing drum, jika terjadi kerusakan segera lakukan penggantian haspel.
* *Finished goods are allowed to be kept outdoor only products that use packing drums.*
* *Duration of storage should not be more than 2 months to avoid rotting wood.*
* *However if it requires storage for more than 2 months then the drum should be painted anti-termite and cover finished goods.*
* *Store finished goods on hard surfaces (casted or paving blocks) that are free from standing water.*
* *Avoid storing on the ground directly because it can make the packing drum become quickly decayed and damaged.*
* *Arrange the finished product drum parallel and can be arranged upward in accordance with SM.08.01.01.*
* *Spread the drums for easy access.Periodic checks are performed to monitor the condition of packing drums, in case of damage immediately do the haspel replacement.*

|  |  |  |
| --- | --- | --- |
| Dibuat oleh  *Made By* | Diperiksa oleh  *Checked By* | Disetujui oleh  *Approved By* |
|  |  |  |
| Mgr. Gudang B. Jadi  *Warehouse FG Manager* | Wakil Manajemen  *MR* | Direktur  *Director* |
|  |  |  |